* GEO-MMS SAASM LIDAR SENSOR

<http://geodetics.com/product/geo-mms-saasm/>

* Prijs op aanvraag
* Sample rate: 125Hz
* Power supply: 10-30V
* Power consumption: >2A
* Single plane scanner (2D)
* Weight: <2.26kg
* Uses VLP-16 PUCK
* LeddarVu

<http://leddartech.com/modules/leddarvu/>

* €520
* Sample rate: 100Hz
* Range: 22m
* Power supply: 12V
* Power consumption: 2W
* Fixed beam, no rotating parts
* Accuracy: 5cm
* Distance precision: 6mm
* Interface options: SPI, USB, CAN, Serial (UART/RS-485)
* Weight: 107g